**Frequently Asked Questions**

**CALL BEFORE YOU DIG**  800-382-5544

**Minimum depth for post holes**  36”

**Temporary pole:**

Need installed, ladder ready DUKE 1-800-774-0246

Lay at site REMC 1-800-737-4111

**Insulation**

Walls R-19

2x6 Foam Board R-15

2x4 Plywood R-13

Attic R-38

**Gas Test Requirements** 10 lbs for 15 minutes

Water 50 lbs for 15 minutes

Drain, waste, vent 5 lbs for 15 minutes

**Expansion tank required**  YES

**When is rail required on deck?**  20 inches

**What is minimum deck rail height?** 3 feet

**Spindle spacing max between**  4 Inches

**Egress window size:**

1st Floor 5 sq ft open

2nd Floor 5.7 sq ft open

**Smoke Detectors –**

Sleeping rooms 1 Each

Outside sleeping rooms 1

Each level of the home 1 Each

No Building Permit Required on Portable Shed

* PLANNING & ZONING NEEDED

No Building Permit required on fencing

* PLANNING & ZONING NEEDED

**Remodel Permit**

No permit required if cosmetic

Permit needed if Structural (ELECTRIC, HVAC, PLUMBING)